sw03#show run

Building configuration...

Current configuration : 1490 bytes

!

! Last configuration change at 00:21:23 UTC Mon Mar 1 1993

!

version 15.0

no service pad

service timestamps debug datetime msec

service timestamps log datetime msec

service password-encryption

!

hostname sw03

!

boot-start-marker

boot-end-marker

!

enable secret 5 $1$4F9j$rzkpwe/NooNpHku88m7Ym/

!

no aaa new-model

system mtu routing 1500

!

!

!

--More--

sw03#show run

Building configuration...

Current configuration : 1490 bytes

!

! Last configuration change at 00:21:23 UTC Mon Mar 1 1993

!

version 15.0

no service pad

service timestamps debug datetime msec

service timestamps log datetime msec

service password-encryption

!

hostname sw03

!

boot-start-marker

boot-end-marker

!

enable secret 5 $1$4F9j$rzkpwe/NooNpHku88m7Ym/

!

no aaa new-model

system mtu routing 1500

!

!

!

--More--

Password:

sw03>

sw03>

sw03>show run

^

% Invalid input detected at '^' marker.

sw03>show run

^

% Invalid input detected at '^' marker.

sw03>enable

Password:

sw03#show run

Building configuration...

Current configuration : 1490 bytes

!

! Last configuration change at 00:21:23 UTC Mon Mar 1 1993

!

version 15.0

no service pad

service timestamps debug datetime msec

service timestamps log datetime msec

service password-encryption

!

hostname sw03

!

boot-start-marker

boot-end-marker

!

enable secret 5 $1$4F9j$rzkpwe/NooNpHku88m7Ym/

!

no aaa new-model

system mtu routing 1500

!

!

!

!

!

!

!

!

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

vlan internal allocation policy ascending

!

!

!

!

!

!

interface FastEthernet0/1

!

interface FastEthernet0/2

!

interface FastEthernet0/3

!

interface FastEthernet0/4

!

interface FastEthernet0/5

!

interface FastEthernet0/6

!

interface FastEthernet0/7

!

interface FastEthernet0/8

!

interface FastEthernet0/9

!

interface FastEthernet0/10

!

interface FastEthernet0/11

!

interface FastEthernet0/12

!

interface FastEthernet0/13

!

interface FastEthernet0/14

!

interface FastEthernet0/15

!

interface FastEthernet0/16

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

!

interface FastEthernet0/22

!

interface FastEthernet0/23

!

interface FastEthernet0/24

!

interface GigabitEthernet0/1

!

interface GigabitEthernet0/2

!

interface Vlan1

ip address 10.16.10.3 255.255.255.0

!

ip http server

ip http secure-server

!

banner motd ^CThis switch is sw03^C

!

line con 0

password 7 060503205F5D

login

line vty 0 4

password 7 060503205F5D

login

line vty 5 15

password 7 060503205F5D

login

!

end